# 

**Acceptance Test Report**

## PN. 4 SN. \_\_\_\_\_\_\_\_ DSP S.N. \_\_\_\_\_\_\_\_ Driver S.N. \_\_\_\_

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Test Name** | **Under Tset** | **Result** | **Pass/Fail** |
| 9.1 | ***Blower Calibration*** | Motor Speed = 8000 ± 100 [RPM]  DRIVER CURRENT = 50 ± 3[A] |  |  |
| 9.2 | ***Functional Test*** | Connect the setup according the figure in parag.7 and Follow procedure presented in the PC according to (P/N – RD-TESTER-0001) 60A DRIVER TESTER test sw.  At the end, add the test file. | |  |
| 10 | ***Cable length*** |  | |  |